**TOPDRY Retracting Line – Grommet Installation Instructions**

**Parts List**

|  |  |  |
| --- | --- | --- |
| AD05527 | Line Hook |  |

**Remove the Line Hook**

|  |  |
| --- | --- |
| **1**  **2** |  |
| 1. Pull out the Front Bar at least 1 metre and extend the line with the Line Hook to be changed an additional 100mm 2. Lock the line tensioner | 1. Unthread the line from the Line Hook to be replaced. |

**Fit the new Line Hook**

|  |  |
| --- | --- |
|  |  |
| 1. Thread the line down through the Line Hook | 1. Loop the line up through the Line Hook |
|  |  |
| 1. Loop the the line over and down | 1. Insert the end of the line in the loop fromed in step 4 and tighten |

Sales Force National Pty Ltd (t/a Zenexus), ABN: 60 110 379 587. Phone: 1300 734 714 (AU), 0800 800 040 (NZ). E-mail: [customerservice@zenexus.com.au](mailto:customerservice@zenexus.com.au)(AU), [customerservice@zenexus.co.nz](mailto:customerservice@zenexus.co.nz) (NZ). Website: [www.zenexus.com.au](http://www.zenexus.com.au)