**TOPDRY Folding Frame – Strut Replacement Installation Instructions**

**Parts List**

|  |  |  |
| --- | --- | --- |
| AD05512 | Strut Assembly - Smoke |  |
| AD05513 | Strut Assembly - Slate |  |

**Remove the Strut to be Replaced**

|  |  |
| --- | --- |
|  |  |
| 1. Unclip the two plastic covers
 | 1. With the frame folded. Remove the screws securing the Strut to the Wall Bracket using two 5mm hex keys
 |

|  |  |
| --- | --- |
|  |  |
| 1. Remove the screws securing the Strut to Arm using two 5mm hex keys.
 | 1. Remove the Strut.
 |

**Fit the replacement strut**

|  |  |
| --- | --- |
|  |  |
| 1. Position the new Strut
 | 1. Assemble and tighten the screws securing the Strut to the Arm
 |

|  |  |
| --- | --- |
|  |  |
| 1. Assemble and tighten the screws securing the Strut to Wall Bracket
 | 1. Clip the plastic covers into position.
 |

Sales Force National Pty Ltd (t/a Zenexus), ABN: 60 110 379 587. Phone: 1300 734 714 (AU), 0800 800 040 (NZ). E-mail: customerservice@zenexus.com.au(AU), customerservice@zenexus.co.nz (NZ). Website: [www.zenexus.com.au](http://www.zenexus.com.au)