**TOPDRY Rotary – Handle Replacement - Installation Instructions**

**Parts List**

|  |  |  |
| --- | --- | --- |
| AD05529 | Handle Assembly - Rotary Evergreen |  |
| AD05530 | Handle Assembly - Rotary Graphite |  |

**Rotary Handle – Removal Instructions**

|  |  |  |
| --- | --- | --- |
|  |  |  |
| 1. Use a small flat bladed screwdrive to remove the two small caps
 | 1. Use a cross head screwdriver to remove the two screws holding the handle to the main post
 | 1. Pull the handle of the square key. Leave the key in place.
 |

**Rotary Handle – Removal Instructions**

|  |  |  |
| --- | --- | --- |
|  |  |  |
| 1. Align the square key with the handle and position the assembly
 | 1. Use a cross head screwdriver to tighten the two screws holding the handle to the main post
 | 1. Push the two caps into position.
 |

Sales Force National Pty Ltd (t/a Zenexus), ABN: 60 110 379 587. Phone: 1300 734 714 (AU), 0800 800 040 (NZ). E-mail: customerservice@zenexus.com.au(AU), customerservice@zenexus.co.nz (NZ). Website: [www.zenexus.com.au](http://www.zenexus.com.au)