**TOPDRY Folding Frame – Corner Replacement Installation Instructions**

**Parts List**

|  |  |  |
| --- | --- | --- |
| AD05518 | Corner- Smoke |  |
| AD05519 | Corner - Slate |  |

**Remove existing Corners**

|  |  |
| --- | --- |
|  |  |
| 1. Remove screw from inside of the Arm. Do this for both sides | 1. Separate the Spreader with the Corners attached from the Arms |

|  |  |
| --- | --- |
|  |  |
| 1. Remove screw from inside of Spreader. Do this for both sides | 1. Pull the corners from the Spreader. |

**Fit new Corner assembly**

|  |  |
| --- | --- |
|  |  |
| 1. Check that the M6 Nyloc nuts are pushed into the Corner part. | 1. Insert the Corners into the Spreader ends, position the Corner Cover and secure with the M6 x 16mm screw. |

|  |  |
| --- | --- |
|  |  |
| 1. Insert the Spreader with the fitted Corners into the arms. | 1. Secure each Corner to each Arms using a M6x16mm screw |

Sales Force National Pty Ltd (t/a Zenexus), ABN: 60 110 379 587. Phone: 1300 734 714 (AU), 0800 800 040 (NZ). E-mail: [customerservice@zenexus.com.au](mailto:customerservice@zenexus.com.au)(AU), [customerservice@zenexus.co.nz](mailto:customerservice@zenexus.co.nz) (NZ). Website: [www.zenexus.com.au](http://www.zenexus.com.au)