**TOPDRY Folding Frame – Handle Replacement Installation Instructions**

**Parts List**

|  |  |  |
| --- | --- | --- |
| AD05520 | Handle - Smoke |  |
| AD05521 | Handle - Slate |  |

**Remove the Handle to be Replaced**

|  |
| --- |
|  |
| 1. Undo the two screws using a 4mm hex key and remove the handle. |
| 1. Position the new handle and secure by tightening the two screws using a 4mm hex key. |

Sales Force National Pty Ltd (t/a Zenexus), ABN: 60 110 379 587. Phone: 1300 734 714 (AU), 0800 800 040 (NZ). E-mail: [customerservice@zenexus.com.au](mailto:customerservice@zenexus.com.au)(AU), [customerservice@zenexus.co.nz](mailto:customerservice@zenexus.co.nz) (NZ). Website: [www.zenexus.com.au](http://www.zenexus.com.au)