**TOPDRY Folding Frame – Coathanger Replacement Installation Instructions**

**Parts List**

|  |  |  |
| --- | --- | --- |
| AD05522 | Coathanger Wire- Smoke |  |
| AD05523 | Coathanger Wire - Slate |  |

**Replace the Coathanger wire**

|  |
| --- |
| **1****3****2** |
| 1. Fold the Coathanger wire to the down position.
 |
| 1. Remove the screws from both sides using a cross head screw driver
 |
| 1. Tilt the wire holder and move outwards to remove – repeat for both sides
 |
| 1. Repeat process in reverse to fit the new parts.
 |

Sales Force National Pty Ltd (t/a Zenexus), ABN: 60 110 379 587. Phone: 1300 734 714 (AU), 0800 800 040 (NZ). E-mail: customerservice@zenexus.com.au(AU), customerservice@zenexus.co.nz (NZ). Website: [www.zenexus.com.au](http://www.zenexus.com.au)